|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Note:   * Orders to operate must be performed in the number sequence listed * A group of operations listed under one sequence number may be performed by any sequence * Apparatus must be in the position stated in “OPERATION” column | | | | | | | |
| Purpose of Order:  **To isolate 54G1 governor electrically under PC14#000624** | | | | | | | |
| **Sequence Number** | **Device** | | **Remove tag no.** | **Operation** | **Place tag no.** | | **initials** |
| 1 | 1B13 | |  | Open |  | |  |
| 2 | 1B14 | |  | Open |  | |  |
| 3 | 1B29 | |  | Open |  | |  |
| 4 | 67S12 | |  | Open |  | |  |
| 5 | 67S13 | |  | Open |  | |  |
| 6 | 67S14 | |  | Open |  | |  |
| 7 | 4S8 | |  | Open and rack out |  | |  |
| 8 | 4S10 | |  | Open and rack out |  | |  |
| 9 | 5S6 | |  | Open and rack out |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
| Prepared By: | | Checked By: | | Ordered By: | | Completed By: | |
| Time: | | Time: | | Time: | | Time: | |
| Date: | | Date: | | Date: | | Date: | |
| Pinboard or Mimic board changed by: | | | | | | | |
|  | | | | PC 2 Serial Number: | | | |

 Serial No.: ……………… Date: ……………………… ORDER TO OPERATE (PC 17) Sheet …………… of ……….......