|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Note:   * Orders to operate must be performed in the number sequence listed * A group of operations listed under one sequence number may be performed by any sequence * Apparatus must be in the position stated in “OPERATION” column | | | | | | | |
| Purpose of Order: **To isolate 54TSS1 at BU54GS** | | | | | | | |
| **Sequence Number** | **Device** | | **Remove tag no.** | **Operation** | | **Place tag no.** | **initials** |
| 1 | 54SS1 Breaker | |  | Check opened and Rack -out | |  |  |
| 2 | 1S2S Breakers | |  | Check Closed | |  |  |
| 3 | 54G1T1 | |  | Check opened and Turn selector switch to local | |  |  |
| 4 | 54T1A breaker | |  | Check opened | |  |  |
| 5 | 54T1A-T | |  | Check opened | |  |  |
| 6 | 54T1-T | |  | Check Opened | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
|  |  | |  |  | |  |  |
| Prepared By: | | Checked By: | | Ordered By: | Completed By: | | |
| Time: | | Time: | | Time: | Time: | | |
| Date: | | Date: | | Date: | Date: | | |
| Pinboard or Mimic board changed by: | | | | | | | |
|  | | | | PC 2 Serial Number: | | | |

 Serial No.: ……………………….. Date: ……………………………….. ORDER TO OPERATE (PC 17) Sheet …………… of ……….......