|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Note:   * Orders to operate must be performed in the number sequence listed * A group of operations listed under one sequence number may be performed by any sequence * Apparatus must be in the position stated in “OPERATION” column | | | | | | | |
| Purpose of Order:  **To de-energize 54G1 Governor under PC14 #001104** | | | | | | | |
| **Sequence Number** | **Device** | | **Remove tag no.** | **Operation** | **Place tag no.** | | **initials** |
| 1 | Pump Selector Switch’s | |  | Turn to off position |  | |  |
| 2 | Air valve selector switch | |  | Turn to stop |  | |  |
| 3 | 1K3K | |  | Close |  | |  |
| 4 | 1K6K | |  | Close |  | |  |
| 5. | 1K8K | |  | Close |  | |  |
| 6. | Air drain valve | |  | Open to drain the air and close |  | |  |
| 7. | 1K2K | |  | Close |  | |  |
| 8. | 1K1K | |  | Close |  | |  |
| 9. | 1K1A | |  | Close |  | |  |
| 10. | 1K1L | |  | Open to drain the oil and close |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
|  |  | |  |  |  | |  |
| Prepared By: | | Checked By: | | Ordered By: | | Completed By: | |
| Time: | | Time: | | Time: | | Time: | |
| Date: | | Date: | | Date: | | Date: | |
| Pinboard or Mimic board changed by: | | | | | | | |
|  | | | | PC 2 Serial Number: | | | |

 Serial No.: ……………………….. Date: ……………………………….. ORDER TO OPERATE (PC 17) Sheet …………… of ……….......